NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Thailand **If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** Thai Industrial Standards Institute (TISI), Ministry of Industry**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** WTO/TBT Enquiry Point and Notification Authority, Thai Industrial Standards Institute (TISI), Ministry of Industry Tel.: (662) 202 3504, 202 3523 Fax: (662) 202 3511, 354 3041 E-mail: thaitbt@tisi.mail.go.th Website: <http://www.tisi.go.th> |
| **3.** | **Notified under Article 2.9.2 [****X], 2.10.1 [ ], 5.6.2 [****X], 5.7.1 [ ], other:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** 29.220.30, 35.020, 35.260 |
| **5.** | **Title, number of pages and language(s) of the notified document:** Thai Industrial Standard for Portable Power Bank – Safety Requirements (TIS 2879-25xx (20xx)) (3 page(s), in Thai)  |
| **6.** | **Description of content:** The Thai Industrial Standards Institute (TISI) has proposed to enforce TIS 2879-25xx (20xx) Portable Power Bank – Safety Requirements as a mandatory standard. The standard covers the safety requirements of portable power bank and any portable energy-storage device containing secondary batteries with charging circuitry via DC output of up to 6 volts, at least one charging port. The standard also includes power bank that supports the external voltage supply for quick charging for electric and electronic devices. In addition, it applies to power bank under intended use and reasonably foreseeable misuse. Excluded from the scope of this standard are: - Any internal battery device that is capable of powering other devices which its main function is not for charging such as portable loudspeaker and laptop - Power bank charged via DC output exceeding 6 volts (e.g. car jump starter) - Uninterruptible power supply (UPS) systemsThe Standard specifies safety requirements, testing, marking and minimum instruction.  |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Safety and consumer protection  |
| **8.** | **Relevant documents:** * TIS 2217: Secondary Cells and Batteries Containing Alkaline or other Non-acid Electrolytes - Safety Requirements for Portable Sealed Secondary Cells, and for Batteries Made from Them, for Use in Portable Applications
* TIS 1561: Information Technology Equipment - Safety - Part 1: General Requirements
 |
| **9.** | **Proposed date of adoption:**To be determined**Proposed date of entry into force:**To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X] or address, telephone and fax numbers and email and website addresses, if available, of other body:** WTO/TBT Enquiry Point and Notification AuthorityThai Industrial Standards InstituteTel: (66 2) 202 3504, 202 3523 Fax: (66 2) 202 3511, 354 3041E-mail: thaitbt@tisi.mail.go.th<https://members.wto.org/crnattachments/2017/TBT/THA/17_4726_00_x.pdf> |